{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":8,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
["ID-10进制","功能说明","长度","读取模式","描述","默认值","备注","ID-16进制"]
[{"$f":"HEX2DEC(H2)","v":256},"读取主机到电脑缓存数据前512",512,"R",null,"00",null,"0100"]
[{"$f":"HEX2DEC(H3)","v":257},"读取主机到电脑缓存数据后512",512,"R",null,"00",null,"0101"]
[258,"读取电脑到主机缓存数据前512",512,"RW",null,"00",null,"0102"]
[259,"读取电脑到主机缓存数据后512",512,"RW",null,"00",null,"0103"]
[260,"读取已存上报数据的点数和未上报的点数",4,"RW",null,"00",null,"0104"]
[261,"读取主机数据解析错误的日志",0,"RW",null,"00",null,"0105"]
[384,"英文字库 T+E+P",18,"W","T:字库类型 byte;E：英文字符 byte;P：对应的点阵 byte[16]","00",null,"0180"]
[385,"中文字库T+C+P",35,"W","T:字库类型 byte;C：中文字符 WORD;P：对应的点阵 byte[32]","00",null,"0181"]
[512,"复位",1,"W","01 终端硬件复位;02 参数区和数据区恢复出厂设置;03参数区恢复出厂设置;04 数据区恢复出厂设置（清除历史数据）","01","BYTE","0200"]
[513,"终端上行通信参数",48,"RW","APN(16字节 STRING)+IP(30字节 STRING)+端口号(WORD)","00","包含APN+IP+PORT/;","0201"]
[514,"终端对时",6,"RW","YY MM DD HH mm SS","101010101010","BCD[6]","0202"]
[515,"终端版本号",13,"R","STRING;设备版本格式：AAAABBCCDDEEN;AAAA: 城市区号，不足补零，如重庆 023 格式为0023;BB：软件生成的年份后两位，如2015，格式为15;CC：主版本号;DD：副版本号;EE：硬件版本号;N:结尾符恒为0","00","包含硬件和软件","0203"]
[516,"心跳间隔 ",1,"RW","BYTE 范围：20-250秒","14","单位:秒","0204"]
[517,"GPRS信号强度",1,"R","1:非常弱     2:弱    3:强    4:非常强","01","BYTE","0205"]
[518,"下发FTP升级参数",92,"W","1-2:端口号 WORD;3-32:IP地址 STRING;33-47:用户名 STRING;48-62:密码 STRING;63-92:升级文件名 STRING","00",null,"0206"]
[519,"串口号+波特率+校验方式+停止位",8,"RW","检验方式：;0x00:USART_Parity_No;0x04:USART_Parity_Even;0x06:USART_Parity_Odd;停止位：;0x00:USART_StopBits_1;0x10:USART_StopBits_0_5;0x20:USART_StopBits_2;0x30:USART_StopBits_1_5;数据长度:;0x00:8;Bits;0x10:9;Bits","00","BYTE+DWORD+BYTE+BYTE+BYTE","0207"]
[520,"终端调试信息输出级别",9,"W","1:级别 BYTE 级别越大输出越多，默认0，只输出系统严重错误信息，范围：0-7，重启后须重新设置，1-5级一级密码;6-7级二级密码，如需设置6-7级须先设置等级到1-5级，再设置6-7级;2-9：密码 string","00",null,"0208"]
[521,"修改信息输出密码",25,"W","1:密码级别，0x5A 一级密码 0xA5 二级密码;2-9：原密码 string;10-17：新密码 string;18-25：新密码 string","00",null,"0209"]
[522,"设置接口类型",1,"RW","1.并口 2.串口","01",null,"020A"]
[523,"下发过滤包",-1,"RW","N<10","31313131",null,"020B"]
[720,"独立烟感报警数据传输",-1,"R","{TABLE_3D0}详情见表","00","III-D-0","02D0"]
[760,"读取设备二维码设备信息",34,"RW","格式：设备类型：字符串 10+分隔号为”:”+设备地址：byte[6]+分隔号+IMEI号：byte[16]如：“ZC1000”：8342443C79EF：31 32 33 34 35 36 37 38","7a4330303030303030303A4442832e833c3Aaa2832e833c4442832e833c4442832ea","针对读取设备二维码设备类型、地址、IMEI","02F8"]
[769,"测量点状态",1,"RW","测量点状态 0：无效；1：有效","01","BYTE","0301"]
[770,"测量点性质",1,"RW","测量点性质：各测量点性质及参数参见表Ⅴ-1","00","BYTE","0302"]
[771,"测量点地址",6,"RW","测量点地址","6662832E833D","BYTE[6]","0303"]
[772,"测量点采集周期",2,"RW","测量点采集周期 单位:分钟 0表示主动上传","0005","WORD","0304"]
[773,"测量点设备参数",4,"RW","{TABLE_5D2}测量点设备参数","00000000","根据测量点性质传输数据,各测量点性质及参数参见表表Ⅴ-2","0305"]
[774,"气体传感器电源自动关闭功能",1,"RW","气体传感器电源自动关闭功能,适用于ZC9000S","01","1-使能自动关闭功能 0-禁止自动关闭功能","0306"]
[775,"气体传感器电源开关控制",1,"RW","气体传感器电源开关控制，适用于ZC9000S","01","1-电源打开 0-电源关闭（后台只能设置电源打开，电源关闭由设备检测到告警后关闭）","0307"]
[776,"气体传感器告警关闭电源超时值",2,"RW","气体传感器告警关闭电源超时值，适用于ZC9000S","0003","时间值，单位为分钟，最小值为1分钟。","0308"]
[777,"液位告警上限和下限",4,"RW","{TABLE_5D4}液位告警上限和下限，适用于ZC9000L","00100002","深度值，见表Ⅴ-4","0309"]
[778,"设备告警触发重置",-1,"W","设备告警触发重置","abab","设备收到该命令后，会恢复之前的告警标记，重新检测告警并上发。","030a"]
[1024,"上报DTU和报警控制器的异常通信状态",7,"RW","上报DTU和报警控制器的异常通信状态，包含无通信和通信异常，不需回复，每隔10分钟上报一次，直至恢复通信","00","时间6字节;状态一字节，共8位;Bit0：CRT->报警控制器无通信;Bit1：报警控制器->CRT无通信;Bit3：帧结构解析错误","0400"]
[1025,"透传当前数据",-1,"RW","透传当前数据","00","BYTE[N]","0401"]
[1026,"透传历史数据",-1,"RW","透传历史数据 ;点数+数据1+……..+数据N","00","BYTE +BYTE[N]","0402"]
[1027,"透传当前数据",-1,"RW","透传当前数据","00","BYTE[N]  N<=512","0403"]
[1281,"上报压力",2,"R","WORD","0001",null,"0501"]
[1282,"告警事件",8,"R","{TABLE_5D3}时间6位+告警标志位2位,见表V-3","1010101010100001",null,"0502"]
[1537,"主机CRT口数据事件",-1,"R","{TABLE_6D1}见表Ⅳ-1","00",null,"0601"]
[1538,"主机打印机口数据事件",-1,"R","{TABLE_6D2}见表Ⅳ-2","00",null,"0602"]
[1793,"液位数据（只支持主动上报）",8,"R","{TABLE_6D2}见表Ⅳ-3","00",null,"0701"]
[1794,"液位告警上传（只支持主动上报）",9,"R","{TABLE_6D2}见表Ⅳ-4","00",null,"0702"]